| Figure 71: DTD-diagram for FM-FUNCTION
Child elements | <long-name> <short-name> <desc> <fm-function-class> <admin-data> <fm-function-type-ref> <fm-prerequisites> <fm-fault-refs>
parent elements | <fm-functions>
Attributes for FM-FUNCTION
Name | Type | Class | Value | Remark
--- | --- | --- | --- | ---
[F-ID-CLASS] | name | fixed | FM-FUNCTION |
[ID] | id | required |  |
[S] | cdata | implied |  |
[T] | cdata | implied |  |
Description Each FM-Function is anchored at one systemelement (FM-Structure-Element). All the functions should describe the aim of their systemelement. Each function is an instance of its type (FM-Function-Type) and may be referenced by FM-Function-Ref.