| Figure 197: DTD-diagram for SW-PARAM-CONTENT-V
Child elements | <sw-unit-ref> <sw-param-values-phys> <sw-param-values-coded> <sw-param-values-coded-hex> <sw-param-values-adr> <sw-param-values-generic>
parent elements | <sw-param-content>
Attributes for SW-PARAM-CONTENT-V
Name | Type | Class | Value | Remark
--- | --- | --- | --- | ---
[S] | cdata | implied |  |
Description An individual value is given here for a characteristic value. The values of the v axis are given here for a characteristic. The values of the v axis are given here for a map. The following convention thereby applies: Index of the x axis runs faster. Values are separated by blanks or line feeds. Example
    <sw-param-content-v>
       <sw-unit-ref>dez</sw-unit-ref>
          <sw-param-values-phys>
             <v>1.000000</v><v>2.000000</v><v>3.000000</v><v>4.000000</v><v>5.000000</v><v>6.000000</v>
       </sw-param-values-phys>
    </sw-param-content-v>