| Figure 58: DTD-diagram for FM-FAULT
Child elements | <long-name> <short-name> <desc> <admin-data> <fm-fault-class> <fm-fault-type-ref> <fm-causes> <fm-significance> <fm-task-history>
parent elements | <fm-faults>
Attributes for FM-FAULT
Name | Type | Class | Value | Remark
--- | --- | --- | --- | ---
[F-ID-CLASS] | name | fixed | FM-FAULT |
[F-NAMESPACE] | names | fixed | FM-TASK-SET FM-TASK-SETS |
[ID] | id | required |  |
[S] | cdata | implied |  |
[T] | cdata | implied |  |
Description FM-Faults are the (possible) failures of Fm-Functions. Each Fm-Fault may have a significance, which is used to compute the risk-priority-factor. The Fm-Fault holds the Fm-Chg element, which is the root to the Fm-Tasks and further to the Fm-Actions.