| Figure 186: DTD-diagram for SW-LIMITS
Child elements | <phys> <coded> <coded> <phys>
parent elements | <sw-axis-individual> <sw-param-axis-values> <sw-physic-type> <sw-physic-type-1> <sw-variable-implementation>
Attributes for SW-LIMITS
Name | Type | Class | Value | Remark
--- | --- | --- | --- | ---
[S] | cdata | implied |  |
Description Minimum and maximum values for the physical and the control-unit-internal values are given here. Example
    <sw-variable-implementation>
       <sw-base-type>UBYTE</sw-base-type>
       <sw-limits>
          <phys>
             <phys-min>40.000000</phys-min>
             <phys-max>4000.000000</phys-max>
          </phys>
       </sw-limits>
          ...
    </sw-variable-implementation>