| Figure 155: DTD-diagram for SW-COMPU-METHOD
Child elements | <admin-data> <long-name> <short-name> <sw-unit-ref> <sw-asap-6-prm-method> <sw-compu-method-table> <sw-compu-method-text> <prog-code> <sw-compu-generic-math>
parent elements | <sw-compu-methods>
Attributes for SW-COMPU-METHOD
Name | Type | Class | Value | Remark
--- | --- | --- | --- | ---
[F-ID-CLASS] | name | fixed | SW-COMPU-METHOD |
[ID] | id | required |  |
[S] | cdata | implied |  |
Description Conversion formula. Computing procedure according to which a control-unit-internal variable can be converted into its physical value. The conversion formula must be reversible. Example